set_location_assignment PIN_11 -to IO11
set_location_assignment PIN_12 -to IO12
set_location_assignment PIN_43 -to clock
set_location_assignment PIN_14 -to IO14
set_location_assignment PIN_16 -to IO16
set_location_assignment PIN_17 -to IO17
set_location_assignment PIN_18 -to IO18
set_location_assignment PIN_19 -to IO19
set_location_assignment PIN_20 -to IO20
set_location_assignment PIN_21 -to IO21
set_instance_assignment -name IO_STANDARD TTL -to IO21
set_location_assignment PIN_24 -to IO24
set_instance_assignment -name IO_STANDARD TTL -to IO24
set_location_assignment PIN_25 -to IO25
set_instance_assignment -name IO_STANDARD TTL -to IO25
set_location_assignment PIN_26 -to IO26
set_instance_assignment -name IO_STANDARD TTL -to IO26
set_instance_assignment -name IO_STANDARD TTL -to IO20
set_instance_assignment -name IO_STANDARD TTL -to IO16
set_instance_assignment -name IO_STANDARD TTL -to IO17
set_instance_assignment -name IO_STANDARD TTL -to IO18
set_instance_assignment -name IO_STANDARD TTL -to IO19
set_instance_assignment -name IO_STANDARD TTL -to IO14
set_location_assignment PIN_5 -to IO5
set_instance_assignment -name IO_STANDARD TTL -to IO5
set_location_assignment PIN_6 -to IO6
set_instance_assignment -name IO_STANDARD TTL -to IO6
set_location_assignment PIN_8 -to IO8
set_instance_assignment -name IO_STANDARD TTL -to IO8
set_location_assignment PIN_9 -to IO9
set_instance_assignment -name IO_STANDARD TTL -to IO9
set_instance_assignment -name IO_STANDARD TTL -to IO11
set_instance_assignment -name IO_STANDARD TTL -to IO12
set_location_assignment PIN_27 -to IO27
set_instance_assignment -name IO_STANDARD TTL -to IO27
set_location_assignment PIN_28 -to IO28
set_instance_assignment -name IO_STANDARD TTL -to IO28
set_location_assignment PIN_29 -to IO29
set_instance_assignment -name IO_STANDARD TTL -to IO29
set_location_assignment PIN_31 -to IO31
set_instance_assignment -name IO_STANDARD TTL -to IO31
set_location_assignment PIN_32 -to TCK
set_location_assignment PIN_13 -to TMS
set_location_assignment PIN_38 -to TDO
set_location_assignment PIN_7 -to TDI
set_location_assignment PIN_33 -to IO33
set_location_assignment PIN_34 -to IO34
set_instance_assignment -name IO_STANDARD TTL -to IO34
set_location_assignment PIN_36 -to IO36
set_instance_assignment -name IO_STANDARD TTL -to IO36
set_location_assignment PIN_37 -to IO37
set_instance_assignment -name IO_STANDARD TTL -to IO37
set_location_assignment PIN_39 -to IO39
set_instance_assignment -name IO_STANDARD TTL -to IO39
set_location_assignment PIN_40 -to IO40
set_location_assignment PIN_41 -to IO41
set_location_assignment PIN_44 -to OE
set_location_assignment PIN_1 -to CLR
set_location_assignment PIN_2 -to I2
set_location_assignment PIN_4 -to IO4
set_instance_assignment -name IO_STANDARD TTL -to IO4
set_global_assignment -name FAMILY MAX7000S
set_global_assignment -name DEVICE "EPM7064SLC44-10"
set_global_assignment -name TOP_LEVEL_ENTITY block1
set_global_assignment -name ORIGINAL_QUARTUS_VERSION "9.1 SP2"
set_global_assignment -name PROJECT_CREATION_TIME_DATE "19:04:47  OCTOBER 03, 2015"
set_global_assignment -name LAST_QUARTUS_VERSION "9.1 SP2"
set_global_assignment -name USE_GENERATED_PHYSICAL_CONSTRAINTS OFF -section_id eda_blast_fpga
set_global_assignment -name MISC_FILE "S:/CPLD/Simple CPLD 64/R1/U1 - Design/SImple-CPLD-Demo.dpf"
set_global_assignment -name SEARCH_PATH "O:/2015/October/CPLD/project/uart2spi/trunk/rtl"
set_global_assignment -name DEVICE_FILTER_PACKAGE ANY
set_global_assignment -name DEVICE_FILTER_PIN_COUNT ANY
set_global_assignment -name DEVICE_FILTER_SPEED_GRADE ANY
set_global_assignment -name VERILOG_FILE block1.v
set_global_assignment -name INCREMENTAL_COMPILATION OFF
